# Allow Tachyon service to access the GXP device and read GXP properties.
allow edgetpu_tachyon_server gxp_device:chr_file rw_file_perms;
get_prop(edgetpu_tachyon_server, vendor_gxp_prop)

# Allow tachyon service to log to stats service for reporting metrics.
allow edgetpu_tachyon_server fwk_stats_service:service_manager find;
binder_call(edgetpu_tachyon_server, system_server);
