set_prop(radio, telephony_ril_prop)

allow radio hal_exynos_rild_hwservice:hwservice_manager find;
allow radio proc_vendor_sched:dir r_dir_perms;
allow radio proc_vendor_sched:file w_file_perms;

# Allow telephony to access file descriptor of the QOS socket
# so it can make sure the QOS is meant for the intended addresses
allow radio priv_app:tcp_socket { read write };
